===============================================================================
LANSchool V3.2

         This file contains instructions for installing LANSchool V3.2.
         There is some user intervention required during the
         installation.  Therefore, please read and follow the directions
         carefully.

         During the installation of LANSchool V3.2, you will be prompted
         to answer a few questions.  These questions will check to see
         where your previous version (3.0 or 3.01) of LANSchool is
         installed and therefore, where you would like to have V3.2
         loaded.

   NOTE: After the system has installed the LANSchool software,
               you must perform the following steps to complete
               installation:

         1) Once the installation is complete, you will be returned to
            the SYSOP's main menu.

         2) Select Modify Program Options.

         3) Select Courseware.

         4) You will see a list of courseware that is currently on your
            server.  The previous version of LANSchool will appear in
            that list.  Tab down to that version (3.0 or 3.01) and
            select it.

         5) The .ITM file for the LANSchool program will appear.  Tab
            down to the Program Description field and change the version
            to V3.2.  Press F10 twice to save and confirm your changes.

         6) All appearances of LANSchool will now show as V3.2.  All
            users who had LANSchool loaded will now have the 3.2 version
            available to them.


    NOTE:  The following is a detailed description of changes in
           LANSchool V3.2

         Bug Fixes:  The Teacher's mouse pointer will be properly
                     restored after the removal of the Teacher's pointer
                     arrow. (This was especially a problem with
                     Microsoft Works)

         Color Information is correctly updated in all video modes.  EGA
         equipment still has trouble if the EGA registers are not
         readable.  If you wish to disable the updating of color data,
         the NOCOLOR switch is available on TEACHER.COM, STUDENT.COM,
         and PEEK.COM.

         Certain older PC-Type student machines would not properly
         receive keystrokes from a teacher while being Peeked.  There
         is a new switch for STUDENT.COM, "KEY_STUFF", which will use a
         different method of keystroke stuffing for older IBM-PC Clones.


         Enhancements: In the default mode, the teacher will send
         graphics screens about 30% faster than older version.  However,
         it is possible to boost this speed even more.  The BURST option
         for TEACHER.COM allows the user to specify how many screen
         packets to send during every Clock Tick.  The default is one
         packet per tick, but this can be increased to 2 or 3. i.e.
         TEACHER BURST=3 will specify 3 screen packets to be sent in
         every clock tick.  This will effectively triple the student
         screen update rate.  However, the larger the BURST number, the
         greater the network traffic.  It is recommended the users who
         wish to operate at a higher BURST rate, experiment with both
         BURST=2 and BURST=3 to see if the network performance remains
         acceptable.

         The memory overhead for LANSchool decreased for both the
         teacher and student modules.  Although this memory decrease is
         not significant, it's always nice to get new features and
         require less memory at the same time!

         






