===============================================================================
PRIMARY EDITOR PLUS VERSION  1.03  -  PROGRAM ENHANCEMENTS

The "Primary Editor Plus" Version 1.03 Program diskette and Tutorial and
Utility diskette include support for the following speech adapters:

    - Digispeech* DS201 and DS201A Speech and Music Units  (*Digispeech
      is a trademark of Digispeech, Inc.)
    - IBM M-Audio Capture and Playback Adapter (M-ACPA)
    - IBM PS/2* Speech Adapter (*PS/2 and Personal System/2 are reg-
      istered trademarks of International Business Machines Corporation.)

Effective with "Primary Editor Plus" Version 1.03, the following
information replaces and supersedes the section entitled, "Specified
Operating Environment" on pages 3 and 4 of the "License Information."

Machine Requirements

Any IBM PS/2 computer with the following minimum configuration:

    - One 3.5-inch diskette drive
    - 640 KB of memory
    - Speech support appropriate for the computer (either the Digispeech*
      DS201 Audio Speech Unit, the IBM M-Audio Capture and Playback
      Adapter, or the IBM Personal System/2* Speech Adapter)

      OPTIONAL: Voice also is available through the system speaker if no
      audio unit or adapter is connected to the computer.

    - Personal System/2* color display is recommended

Any printer capable of running in the IBM Personal Printer Data Stream
(PPDS) mode (optional)

This update contains modified instructions to install on a network

INSTALLING "PRIMARY EDITOR PLUS" ON IBM CLASSROOM LAN ADMINISTRATION
SYSTEM

NOTE:  This procedure is for a system administrator (user ID ADMIN).
Follow these steps to install Primary Editor Plus on the network:

  1.  From a workstation, log in as a SYSOP or ADMIN ID.

  2.  Change current drive to CD-ROM drive.

  3.  Type "INSTALL" and hit Enter.  Hit Space Bar to view
      the instructions.

  4.  Select "Selectively Install Updates" from the Patch Update Main Menu.

  5.  Select "Primary Editor Plus V1.03"

      The installation procedure may ask you what volume to install the update.
      Select the volume of your choice.

      After a short amount of time, the program will be installed, and the
      Patch Update Main Menu appears.

IMPORTANT:
If you are using remote boot with DOS 3.30, you must do the following:

    1. Replace the GRAPHICS.COM file on the remote boot image disk with
       the GRAPHICS.COM and GRAPHICS.PRO files included on the "Primary
       Editor Plus" Program diskette.
    2. Use the NetWare* DOSGEN program to create a remote boot image.
       *(NetWare is a registered trademark of Novell, Inc.)
       
                                                                                
CHANGES AND MODIFICATIONS

  This file contains notices concerning changes or updates made to the          
  Primary Editor Plus, version 1.03 package (PEP103).                           
                                                                                
  Any changes made to PEP103 after the initial release (10/20/92) are           
  documented in this file.                                                      
                                                                                
                                                                                
  10/20/92 - Change List:                                                       
  -----------------------                                                       
                                                                                
  1.  Print creeping patch was added.                                           
                                                                                
  2.  386 voice patch was added to both the program and tutorial                
      diskettes.  Previous to this version voice would not be available         
      on 386 processor machines.                                                
                                                                                
  3.  The PEP item file was modified to include a call to the UP utility        
      necessary for ICLAS 1.4 so that the ICLAS CLS?.USE file was               
      converted to the format that PEP recognizes.                              
                                                                                
  4.  A start-up speech device recognition program detects which of the         
      following speech devices is attached to the work station and              
      accordingly load the speech driver.                                       
           - Digispeech                                                         
           - M-ACPA                                                             
           - IBM Speech Adapter                                                 
                                                                                
  5.  Regular DOS v3.30 system programming instead of booter loader.            
                                                                                
  6.  Hardfile install\uninstall utility which is found on the Tutorial         
      diskette.  The Install Utility asks the user whether to install           
      the program or tutorial and makes the necessary prompts for the           
      program diskette if chosen.                                               
                                                                                
  Note:  Use of the PEPPRINT PACKAGE on ESMS Tools may still be                 
      necessary as it contains optional double\high\wide\modes for              
      printing that could not be included with the new release since            
      it is user preference.

















